.. _mimxrt1050_evk:

NXP MIMXRT1050-EVK
##################

Overview
********

The i.MX RT1050 is a new processor family featuring NXP's advanced
implementation of the ARM Cortex-M7 Core. It provides high CPU performance and
real-time response.

The i.MX RT1050 provides various memory interfaces, including SDRAM, Raw NAND
FLASH, NOR FLASH, SD/eMMC, Quad SPI, HyperBus and a wide range of other
interfaces for connecting peripherals, such as WLAN, Bluetooth™, GPS, displays,
and camera sensors. As with other i.MX processors, i.MX RT1050 also has rich
audio and video features, including LCD display, basic 2D graphics, camera
interface, SPDIF, and I2S audio interface.

The following document refers to the discontinued MIMXRT1050-EVK board. For the
MIMXRT1050-EVKB board, refer to `Board Revisions`_ section.

.. image:: ./mimxrt1050_evk.jpg
   :width: 720px
   :align: center
   :alt: MIMXRT1050-EVK

Hardware
********

- MIMXRT1052DVL6A MCU (600 MHz, 512 KB TCM)

- Memory

  - 256 KB SDRAM
  - 64 Mbit QSPI Flash
  - 512 Mbit Hyper Flash

- Display

  - LCD connector
  - Touch connector

- Ethernet

  - 10/100 Mbit/s Ethernet PHY

- USB

  - USB 2.0 OTG connector
  - USB 2.0 host connector

- Audio

  - 3.5 mm audio stereo headphone jack
  - Board-mounted microphone
  - Left and right speaker out connectors

- Power

  - 5 V DC jack

- Debug

  - JTAG 20-pin connector
  - OpenSDA with DAPLink

- Sensor

  - FXOS8700CQ 6-axis e-compass
  - CMOS camera sensor interface

- Expansion port

  - Arduino interface

- CAN bus connector

For more information about the MIMXRT1050 SoC and MIMXRT1050-EVK board, see
these references:

- `i.MX RT1050 Website`_
- `i.MX RT1050 Datasheet`_
- `i.MX RT1050 Reference Manual`_
- `MIMXRT1050-EVK Website`_
- `MIMXRT1050-EVK User Guide`_
- `MIMXRT1050-EVK Schematics`_

Supported Features
==================

The mimxrt1050_evk board configuration supports the following hardware
features:

+-----------+------------+-------------------------------------+
| Interface | Controller | Driver/Component                    |
+===========+============+=====================================+
| NVIC      | on-chip    | nested vector interrupt controller  |
+-----------+------------+-------------------------------------+
| SYSTICK   | on-chip    | systick                             |
+-----------+------------+-------------------------------------+
| DISPLAY   | on-chip    | display                             |
+-----------+------------+-------------------------------------+
| GPIO      | on-chip    | gpio                                |
+-----------+------------+-------------------------------------+
| I2C       | on-chip    | i2c                                 |
+-----------+------------+-------------------------------------+
| SPI       | on-chip    | spi                                 |
+-----------+------------+-------------------------------------+
| UART      | on-chip    | serial port-polling;                |
|           |            | serial port-interrupt               |
+-----------+------------+-------------------------------------+
| ENET      | on-chip    | ethernet                            |
+-----------+------------+-------------------------------------+
| USB       | on-chip    | USB device                          |
+-----------+------------+-------------------------------------+

The default configuration can be found in the defconfig file:

	``boards/arm/mimxrt1050_evk/mimxrt1050_evk_defconfig``

Other hardware features are not currently supported by the port.

Connections and IOs
===================

The MIMXRT1050 SoC has five pairs of pinmux/gpio controllers.

+---------------+-----------------+---------------------------+
| Name          | Function        | Usage                     |
+===============+=================+===========================+
| GPIO_AD_B0_00 | LPSPI3_SCK      | SPI                       |
+---------------+-----------------+---------------------------+
| GPIO_AD_B0_01 | LPSPI3_SDO      | SPI                       |
+---------------+-----------------+---------------------------+
| GPIO_AD_B0_02 | LPSPI3_SDI/LCD_RST| SPI/LCD Display         |
+---------------+-----------------+---------------------------+
| GPIO_AD_B0_03 | LPSPI3_PCS0     | SPI                       |
+---------------+-----------------+---------------------------+
| GPIO_AD_B0_09 | GPIO/ENET_RST   | LED                       |
+---------------+-----------------+---------------------------+
| GPIO_AD_B0_10 | GPIO/ENET_INT   | GPIO/Ethernet             |
+---------------+-----------------+---------------------------+
| GPIO_AD_B0_12 | LPUART1_TX      | UART Console              |
+---------------+-----------------+---------------------------+
| GPIO_AD_B0_13 | LPUART1_RX      | UART Console              |
+---------------+-----------------+---------------------------+
| GPIO_AD_B1_00 | LPI2C1_SCL      | I2C                       |
+---------------+-----------------+---------------------------+
| GPIO_AD_B1_01 | LPI2C1_SDA      | I2C                       |
+---------------+-----------------+---------------------------+
| GPIO_AD_B1_06 | LPUART3_TX      | UART BT HCI               |
+---------------+-----------------+---------------------------+
| GPIO_AD_B1_07 | LPUART3_RX      | UART BT HCI               |
+---------------+-----------------+---------------------------+
| WAKEUP        | GPIO            | SW0                       |
+---------------+-----------------+---------------------------+
| GPIO_B0_00    | LCD_CLK         | LCD Display               |
+---------------+-----------------+---------------------------+
| GPIO_B0_01    | LCD_ENABLE      | LCD Display               |
+---------------+-----------------+---------------------------+
| GPIO_B0_02    | LCD_HSYNC       | LCD Display               |
+---------------+-----------------+---------------------------+
| GPIO_B0_03    | LCD_VSYNC       | LCD Display               |
+---------------+-----------------+---------------------------+
| GPIO_B0_04    | LCD_DATA00      | LCD Display               |
+---------------+-----------------+---------------------------+
| GPIO_B0_05    | LCD_DATA01      | LCD Display               |
+---------------+-----------------+---------------------------+
| GPIO_B0_06    | LCD_DATA02      | LCD Display               |
+---------------+-----------------+---------------------------+
| GPIO_B0_07    | LCD_DATA03      | LCD Display               |
+---------------+-----------------+---------------------------+
| GPIO_B0_08    | LCD_DATA04      | LCD Display               |
+---------------+-----------------+---------------------------+
| GPIO_B0_09    | LCD_DATA05      | LCD Display               |
+---------------+-----------------+---------------------------+
| GPIO_B0_10    | LCD_DATA06      | LCD Display               |
+---------------+-----------------+---------------------------+
| GPIO_B0_11    | LCD_DATA07      | LCD Display               |
+---------------+-----------------+---------------------------+
| GPIO_B0_12    | LCD_DATA08      | LCD Display               |
+---------------+-----------------+---------------------------+
| GPIO_B0_13    | LCD_DATA09      | LCD Display               |
+---------------+-----------------+---------------------------+
| GPIO_B0_14    | LCD_DATA10      | LCD Display               |
+---------------+-----------------+---------------------------+
| GPIO_B0_15    | LCD_DATA11      | LCD Display               |
+---------------+-----------------+---------------------------+
| GPIO_B1_00    | LCD_DATA12      | LCD Display               |
+---------------+-----------------+---------------------------+
| GPIO_B1_01    | LCD_DATA13      | LCD Display               |
+---------------+-----------------+---------------------------+
| GPIO_B1_02    | LCD_DATA14      | LCD Display               |
+---------------+-----------------+---------------------------+
| GPIO_B1_03    | LCD_DATA15      | LCD Display               |
+---------------+-----------------+---------------------------+
| GPIO_B1_04    | ENET_RX_DATA00  | Ethernet                  |
+---------------+-----------------+---------------------------+
| GPIO_B1_05    | ENET_RX_DATA01  | Ethernet                  |
+---------------+-----------------+---------------------------+
| GPIO_B1_06    | ENET_RX_EN      | Ethernet                  |
+---------------+-----------------+---------------------------+
| GPIO_B1_07    | ENET_TX_DATA00  | Ethernet                  |
+---------------+-----------------+---------------------------+
| GPIO_B1_08    | ENET_TX_DATA01  | Ethernet                  |
+---------------+-----------------+---------------------------+
| GPIO_B1_09    | ENET_TX_EN      | Ethernet                  |
+---------------+-----------------+---------------------------+
| GPIO_B1_10    | ENET_REF_CLK    | Ethernet                  |
+---------------+-----------------+---------------------------+
| GPIO_B1_11    | ENET_RX_ER      | Ethernet                  |
+---------------+-----------------+---------------------------+
| GPIO_B1_15    | BACKLIGHT_CTL   | LCD Display               |
+---------------+-----------------+---------------------------+
| GPIO_EMC_40   | ENET_MDC        | Ethernet                  |
+---------------+-----------------+---------------------------+
| GPIO_EMC_41   | ENET_MDIO       | Ethernet                  |
+---------------+-----------------+---------------------------+
| GPIO_AD_B0_09 | ENET_RST        | Ethernet                  |
+---------------+-----------------+---------------------------+
| GPIO_AD_B0_10 | ENET_INT        | Ethernet                  |
+---------------+-----------------+---------------------------+

System Clock
============

The MIMXRT1050 SoC is configured to use the 24 MHz external oscillator on the
board with the on-chip PLL to generate a 600 MHz core clock.

Serial Port
===========

The MIMXRT1050 SoC has eight UARTs. ``LPUART1`` is configured for the console,
``LPUART3`` for the Bluetooth Host Controller Interface (BT HCI), and the
remaining are not used.

USB
===

The RT1050 SoC has two USB OTG (USBOTG) controllers that supports both
device and host functions through its micro USB connectors.
Only USB device function is supported in Zephyr at the moment.

Programming and Debugging
*************************

Build and flash applications as usual (see :ref:`build_an_application` and
:ref:`application_run` for more details).

Configuring a Debug Probe
=========================

A debug probe is used for both flashing and debugging the board. This board is
configured by default to use the :ref:`opensda-daplink-onboard-debug-probe`,
however the :ref:`pyocd-debug-host-tools` do not yet support programming the
external flashes on this board so you must reconfigure the board for one of the
following debug probes instead.

Option 1: :ref:`opensda-jlink-onboard-debug-probe` (Recommended)
----------------------------------------------------------------

Install the :ref:`jlink-debug-host-tools` and make sure they are in your search
path.

Follow the instructions in :ref:`opensda-jlink-onboard-debug-probe` to program
the `OpenSDA J-Link MIMXRT1050-EVK-Hyperflash Firmware`_. Check that jumpers
J32 and J33 are **on** (they are on by default when boards ship from the
factory) to ensure SWD signals are connected to the OpenSDA microcontroller.

Option 2: :ref:`jlink-external-debug-probe`
-------------------------------------------

Install the :ref:`jlink-debug-host-tools` and make sure they are in your search
path.

Attach a J-Link 20-pin connector to J21. Check that jumpers J32 and J33 are
**off** (they are on by default when boards ship from the factory) to ensure
SWD signals are disconnected from the OpenSDA microcontroller.

Configuring a Console
=====================

Regardless of your choice in debug probe, we will use the OpenSDA
microcontroller as a usb-to-serial adapter for the serial console. Check that
jumpers J30 and J31 are **on** (they are on by default when boards ship from
the factory) to connect UART signals to the OpenSDA microcontroller.

Connect a USB cable from your PC to J28.

Use the following settings with your serial terminal of choice (minicom, putty,
etc.):

- Speed: 115200
- Data: 8 bits
- Parity: None
- Stop bits: 1

Flashing
========

Here is an example for the :ref:`hello_world` application.

.. zephyr-app-commands::
   :zephyr-app: samples/hello_world
   :board: mimxrt1050_evk
   :goals: flash

Open a serial terminal, reset the board (press the SW4 button), and you should
see the following message in the terminal:

.. code-block:: console

   ***** Booting Zephyr OS v1.14.0-rc1 *****
   Hello World! mimxrt1050_evk

Debugging
=========

Here is an example for the :ref:`hello_world` application.

.. zephyr-app-commands::
   :zephyr-app: samples/hello_world
   :board: mimxrt1050_evk
   :goals: debug

Open a serial terminal, step through the application in your debugger, and you
should see the following message in the terminal:

.. code-block:: console

   ***** Booting Zephyr OS v1.14.0-rc1 *****
   Hello World! mimxrt1050_evk

Board Revisions
***************

The original MIMXRT1050-EVK (rev A0) board was updated with a newer
MIMXRT1050-EVKB (rev A1) board, with these major hardware differences::

- SoC changed from MIMXRT1052DVL6**A** to MIMXRT1052DVL6**B**
- Hardware bug fixes for: power, interfaces, and memory
- Arduino headers included

For more details, please see the following `NXP i.MXRT1050 A0 to A1 Migration Guide`_.

Current Zephyr build supports the new MIMXRT1050-EVKB

.. _MIMXRT1050-EVK Website:
   https://www.nxp.com/products/microcontrollers-and-processors/arm-based-processors-and-mcus/i.mx-applications-processors/i.mx-rt-series/i.mx-rt1050-evaluation-kit:MIMXRT1050-EVK

.. _MIMXRT1050-EVK User Guide:
   https://www.nxp.com/webapp/Download?colCode=IMXRT1050EVKBHUG

.. _MIMXRT1050-EVK Schematics:
   https://www.nxp.com/webapp/Download?colCode=MIMXRT1050-EVK-DESIGNFILES

.. _i.MX RT1050 Website:
   https://www.nxp.com/products/microcontrollers-and-processors/arm-based-processors-and-mcus/i.mx-applications-processors/i.mx-rt-series/i.mx-rt1050-crossover-processor-with-arm-cortex-m7-core:i.MX-RT1050

.. _i.MX RT1050 Datasheet:
   https://www.nxp.com/docs/en/data-sheet/IMXRT1050CEC.pdf

.. _i.MX RT1050 Reference Manual:
   https://www.nxp.com/docs/en/reference-manual/IMXRT1050RM.pdf

.. _OpenSDA J-Link MIMXRT1050-EVK-Hyperflash Firmware:
   https://www.segger.com/downloads/jlink/OpenSDA_MIMXRT1050-EVK-Hyperflash

.. _NXP i.MXRT1050 A0 to A1 Migration Guide:
   https://www.nxp.com/docs/en/nxp/application-notes/AN12146.pdf
