Name:
=====
 ios_lram


Description:
============
 Example slave used for demonstrating the use of the IOS lram.


Purpose:
========
This slave component runs on one EVB and is used in conjunction with
the companion host example, ios_lram_host, which runs on a second EVB.

Printing takes place over the ITM at 1M Baud.

Additional Information:
=======================
In order to run this example, a host device (e.g. a second EVB) must be set
up to run the host example, ios_lram_host.  The two boards can be connected
using fly leads between the two boards as follows.

Pin connections for the I/O Master board to the I/O Slave board.
SPI:
HOST (ios_lram_host)                    SLAVE (ios_lram)
--------------------                    ----------------
GPIO[10] GPIO Interrupt (slave to host) GPIO[4]  GPIO interrupt
GPIO[5]  IOM0 SPI SCK                   GPIO[0]  IOS SPI SCK
GPIO[7]  IOM0 SPI MOSI                  GPIO[1]  IOS SPI MOSI
GPIO[6]  IOM0 SPI MISO                  GPIO[2]  IOS SPI MISO
GPIO[11] IOM0 SPI nCE                   GPIO[3]  IOS SPI nCE
GND                                     GND

I2C:
HOST (ios_lram_host)                    SLAVE (ios_lram)
--------------------                    ----------------
GPIO[10] GPIO Interrupt (slave to host) GPIO[4]  GPIO interrupt
GPIO[5]  IOM0 I2C SCL                   GPIO[0]  IOS I2C SCL
GPIO[6]  IOM0 I2C SDA                   GPIO[1]  IOS I2C SDA
GND                                     GND


******************************************************************************


