| Apollo Register Documentation v2.2.0

- Main Page

MCUCTRL - MCU Miscellaneous Control Logic

### MCUCTRL Register Index

0x00000000: | CHIP_INFO - Chip Information Register
0x00000004: | CHIPID0 - Unique Chip ID 0
0x00000008: | CHIPID1 - Unique Chip ID 1
0x0000000C: | CHIPREV - Chip Revision
0x00000010: | VENDORID - Unique Vendor ID
0x00000014: | DEBUGGER - Debugger Control
0x0000010C: | ADCCAL - ADC Calibration Control
0x00000110: | ADCBATTLOAD - ADC Battery Load Enable
0x0000011C: | ADCREFCOMP - ADC Referece Keeper and Comparator Control
0x00000124: | XTALGENCTRL - XTAL Oscillator General Control
0x000001A0: | BOOTLOADERLOW - Determines whether the bootloader code is visible at address 0x00000000
0x000001A4: | SHADOWVALID - Register to indicate whether the shadow registers have been successfully loaded from the Flash Information Space.
0x000001C0: | ICODEFAULTADDR - ICODE bus address which was present when a bus fault occurred.
0x000001C4: | DCODEFAULTADDR - DCODE bus address which was present when a bus fault occurred.
0x000001C8: | SYSFAULTADDR - System bus address which was present when a bus fault occurred.
0x000001CC: | FAULTSTATUS - Reflects the status of the bus decoders' fault detection. Any write to this register will clear all of the status bits within the register.
0x000001D0: | FAULTCAPTUREEN - Enable the fault capture registers
0x00000200: | DBGR1 - Read-only debug register 1
0x00000204: | DBGR2 - Read-only debug register 2
0x00000220: | PMUENABLE - Control bit to enable/disable the PMU
0x00000250: | TPIUCTRL - TPIU Control Register. Determines the clock enable and frequency for the M4's TPIU interface.
0x00000348: | KEXTCLKSEL - Key Register to enable the use of external clock selects via the EXTCLKSEL reg

### CHIP_INFO - Chip Information Register

### Address:

Instance 0 Address: | 0x40020000

### Description:

Chip Information Register

### Example Macro Usage:

    //
    // All macro-based register writes follow the same basic format. For
    // single-instance modules, you may use the simpler AM_REG macro. For
    // multi-instance macros, you will need to specify the instance number using
    // the AM_REGn macro format.
    //
    // AM_REG(<MODULE>, <REGISTER>) |= AM_REG_<MODULE>_<REGISTER>_<FIELD>_<VALUE>;
    // AM_REGn(<MODULE>, <INSTANCE>, <REGISTER>) |= AM_REG_<MODULE>_<REGISTER>_<FIELD>_<VALUE>;
    //
    // For registers that do not have specific enumeration values, you may use this alternate format instead.
    //
    // AM_REG(<MODULE>, <REGISTER>) |= AM_REG_<MODULE>_<REGISTER>_<FIELD>(<NUMBER>);
    //
    // For example, the following three lines of code are equivalent methods of
    // writing the value for 12MHZ to the CLKSEL field in the ADC_CFG register.
    //
    AM_REG(ADC, CFG) |= AM_REG_ADC_CFG_CLKSEL_12MHZ;
    AM_REGn(ADC, 0, CFG) |= AM_REG_ADC_CFG_CLKSEL_12MHZ;
    AM_REG(ADC, CFG) |= AM_REG_ADC_CFG_CLKSEL(0x1);

### Register Fields:

31 | 30 | 29 | 28 | 27 | 26 | 25 | 24 | 23 | 22 | 21 | 20 | 19 | 18 | 17 | 16 | 15 | 14 | 13 | 12 | 11 | 10 | 9 | 8 | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0
--- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | ---
PARTNUM 0x0

Bits | Name | RW | Description
--- | --- | --- | ---
31:0 | PARTNUM | RO | BCD part number. APOLLO2 = 0x0 - Apollo2 part number.

### CHIPID0 - Unique Chip ID 0

### Address:

Instance 0 Address: | 0x40020004

### Description:

Unique Chip ID 0

### Example Macro Usage:

    //
    // All macro-based register writes follow the same basic format. For
    // single-instance modules, you may use the simpler AM_REG macro. For
    // multi-instance macros, you will need to specify the instance number using
    // the AM_REGn macro format.
    //
    // AM_REG(<MODULE>, <REGISTER>) |= AM_REG_<MODULE>_<REGISTER>_<FIELD>_<VALUE>;
    // AM_REGn(<MODULE>, <INSTANCE>, <REGISTER>) |= AM_REG_<MODULE>_<REGISTER>_<FIELD>_<VALUE>;
    //
    // For registers that do not have specific enumeration values, you may use this alternate format instead.
    //
    // AM_REG(<MODULE>, <REGISTER>) |= AM_REG_<MODULE>_<REGISTER>_<FIELD>(<NUMBER>);
    //
    // For example, the following three lines of code are equivalent methods of
    // writing the value for 12MHZ to the CLKSEL field in the ADC_CFG register.
    //
    AM_REG(ADC, CFG) |= AM_REG_ADC_CFG_CLKSEL_12MHZ;
    AM_REGn(ADC, 0, CFG) |= AM_REG_ADC_CFG_CLKSEL_12MHZ;
    AM_REG(ADC, CFG) |= AM_REG_ADC_CFG_CLKSEL(0x1);

### Register Fields:

31 | 30 | 29 | 28 | 27 | 26 | 25 | 24 | 23 | 22 | 21 | 20 | 19 | 18 | 17 | 16 | 15 | 14 | 13 | 12 | 11 | 10 | 9 | 8 | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0
--- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | ---
VALUE 0x0

Bits | Name | RW | Description
--- | --- | --- | ---
31:0 | VALUE | RO | Unique chip ID 0. APOLLO2 = 0x0 - Apollo2 CHIPID0.

### CHIPID1 - Unique Chip ID 1

### Address:

Instance 0 Address: | 0x40020008

### Description:

Unique Chip ID 1

### Example Macro Usage:

    //
    // All macro-based register writes follow the same basic format. For
    // single-instance modules, you may use the simpler AM_REG macro. For
    // multi-instance macros, you will need to specify the instance number using
    // the AM_REGn macro format.
    //
    // AM_REG(<MODULE>, <REGISTER>) |= AM_REG_<MODULE>_<REGISTER>_<FIELD>_<VALUE>;
    // AM_REGn(<MODULE>, <INSTANCE>, <REGISTER>) |= AM_REG_<MODULE>_<REGISTER>_<FIELD>_<VALUE>;
    //
    // For registers that do not have specific enumeration values, you may use this alternate format instead.
    //
    // AM_REG(<MODULE>, <REGISTER>) |= AM_REG_<MODULE>_<REGISTER>_<FIELD>(<NUMBER>);
    //
    // For example, the following three lines of code are equivalent methods of
    // writing the value for 12MHZ to the CLKSEL field in the ADC_CFG register.
    //
    AM_REG(ADC, CFG) |= AM_REG_ADC_CFG_CLKSEL_12MHZ;
    AM_REGn(ADC, 0, CFG) |= AM_REG_ADC_CFG_CLKSEL_12MHZ;
    AM_REG(ADC, CFG) |= AM_REG_ADC_CFG_CLKSEL(0x1);

### Register Fields:

31 | 30 | 29 | 28 | 27 | 26 | 25 | 24 | 23 | 22 | 21 | 20 | 19 | 18 | 17 | 16 | 15 | 14 | 13 | 12 | 11 | 10 | 9 | 8 | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0
--- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | ---
VALUE 0x0

Bits | Name | RW | Description
--- | --- | --- | ---
31:0 | VALUE | RO | Unique chip ID 1. APOLLO2 = 0x0 - Apollo2 CHIPID1.

### CHIPREV - Chip Revision

### Address:

Instance 0 Address: | 0x4002000C

### Description:

Chip Revision

### Example Macro Usage:

    //
    // All macro-based register writes follow the same basic format. For
    // single-instance modules, you may use the simpler AM_REG macro. For
    // multi-instance macros, you will need to specify the instance number using
    // the AM_REGn macro format.
    //
    // AM_REG(<MODULE>, <REGISTER>) |= AM_REG_<MODULE>_<REGISTER>_<FIELD>_<VALUE>;
    // AM_REGn(<MODULE>, <INSTANCE>, <REGISTER>) |= AM_REG_<MODULE>_<REGISTER>_<FIELD>_<VALUE>;
    //
    // For registers that do not have specific enumeration values, you may use this alternate format instead.
    //
    // AM_REG(<MODULE>, <REGISTER>) |= AM_REG_<MODULE>_<REGISTER>_<FIELD>(<NUMBER>);
    //
    // For example, the following three lines of code are equivalent methods of
    // writing the value for 12MHZ to the CLKSEL field in the ADC_CFG register.
    //
    AM_REG(ADC, CFG) |= AM_REG_ADC_CFG_CLKSEL_12MHZ;
    AM_REGn(ADC, 0, CFG) |= AM_REG_ADC_CFG_CLKSEL_12MHZ;
    AM_REG(ADC, CFG) |= AM_REG_ADC_CFG_CLKSEL(0x1);

### Register Fields:

31 | 30 | 29 | 28 | 27 | 26 | 25 | 24 | 23 | 22 | 21 | 20 | 19 | 18 | 17 | 16 | 15 | 14 | 13 | 12 | 11 | 10 | 9 | 8 | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0
--- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | ---
RSVD 0x0 | REVMAJ 0x1 | REVMIN 0x1

Bits | Name | RW | Description
--- | --- | --- | ---
31:8 | RSVD | RO | RESERVED.
7:4 | REVMAJ | RO | Major Revision ID. A = 0x1 - Apollo2 revision A
3:0 | REVMIN | RO | Minor Revision ID. REV0 = 0x1 - Apollo2 minor revision value.

### VENDORID - Unique Vendor ID

### Address:

Instance 0 Address: | 0x40020010

### Description:

Unique Vendor ID

### Example Macro Usage:

    //
    // All macro-based register writes follow the same basic format. For
    // single-instance modules, you may use the simpler AM_REG macro. For
    // multi-instance macros, you will need to specify the instance number using
    // the AM_REGn macro format.
    //
    // AM_REG(<MODULE>, <REGISTER>) |= AM_REG_<MODULE>_<REGISTER>_<FIELD>_<VALUE>;
    // AM_REGn(<MODULE>, <INSTANCE>, <REGISTER>) |= AM_REG_<MODULE>_<REGISTER>_<FIELD>_<VALUE>;
    //
    // For registers that do not have specific enumeration values, you may use this alternate format instead.
    //
    // AM_REG(<MODULE>, <REGISTER>) |= AM_REG_<MODULE>_<REGISTER>_<FIELD>(<NUMBER>);
    //
    // For example, the following three lines of code are equivalent methods of
    // writing the value for 12MHZ to the CLKSEL field in the ADC_CFG register.
    //
    AM_REG(ADC, CFG) |= AM_REG_ADC_CFG_CLKSEL_12MHZ;
    AM_REGn(ADC, 0, CFG) |= AM_REG_ADC_CFG_CLKSEL_12MHZ;
    AM_REG(ADC, CFG) |= AM_REG_ADC_CFG_CLKSEL(0x1);

### Register Fields:

31 | 30 | 29 | 28 | 27 | 26 | 25 | 24 | 23 | 22 | 21 | 20 | 19 | 18 | 17 | 16 | 15 | 14 | 13 | 12 | 11 | 10 | 9 | 8 | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0
--- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | ---
VALUE 0x0

Bits | Name | RW | Description
--- | --- | --- | ---
31:0 | VALUE | RO | Unique Vendor ID AMBIQ = 0x414D4251 - Ambiq Venfor ID

### DEBUGGER - Debugger Control

### Address:

Instance 0 Address: | 0x40020014

### Description:

Debugger Control

### Example Macro Usage:

    //
    // All macro-based register writes follow the same basic format. For
    // single-instance modules, you may use the simpler AM_REG macro. For
    // multi-instance macros, you will need to specify the instance number using
    // the AM_REGn macro format.
    //
    // AM_REG(<MODULE>, <REGISTER>) |= AM_REG_<MODULE>_<REGISTER>_<FIELD>_<VALUE>;
    // AM_REGn(<MODULE>, <INSTANCE>, <REGISTER>) |= AM_REG_<MODULE>_<REGISTER>_<FIELD>_<VALUE>;
    //
    // For registers that do not have specific enumeration values, you may use this alternate format instead.
    //
    // AM_REG(<MODULE>, <REGISTER>) |= AM_REG_<MODULE>_<REGISTER>_<FIELD>(<NUMBER>);
    //
    // For example, the following three lines of code are equivalent methods of
    // writing the value for 12MHZ to the CLKSEL field in the ADC_CFG register.
    //
    AM_REG(ADC, CFG) |= AM_REG_ADC_CFG_CLKSEL_12MHZ;
    AM_REGn(ADC, 0, CFG) |= AM_REG_ADC_CFG_CLKSEL_12MHZ;
    AM_REG(ADC, CFG) |= AM_REG_ADC_CFG_CLKSEL(0x1);

### Register Fields:

31 | 30 | 29 | 28 | 27 | 26 | 25 | 24 | 23 | 22 | 21 | 20 | 19 | 18 | 17 | 16 | 15 | 14 | 13 | 12 | 11 | 10 | 9 | 8 | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0
--- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | ---
RSVD 0x0 | LOCKOUT 0x0

Bits | Name | RW | Description
--- | --- | --- | ---
31:1 | RSVD | RO | RESERVED
0 | LOCKOUT | RW | Lockout of debugger (SWD).

### ADCCAL - ADC Calibration Control

### Address:

Instance 0 Address: | 0x4002010C

### Description:

ADC Calibration Control

### Example Macro Usage:

    //
    // All macro-based register writes follow the same basic format. For
    // single-instance modules, you may use the simpler AM_REG macro. For
    // multi-instance macros, you will need to specify the instance number using
    // the AM_REGn macro format.
    //
    // AM_REG(<MODULE>, <REGISTER>) |= AM_REG_<MODULE>_<REGISTER>_<FIELD>_<VALUE>;
    // AM_REGn(<MODULE>, <INSTANCE>, <REGISTER>) |= AM_REG_<MODULE>_<REGISTER>_<FIELD>_<VALUE>;
    //
    // For registers that do not have specific enumeration values, you may use this alternate format instead.
    //
    // AM_REG(<MODULE>, <REGISTER>) |= AM_REG_<MODULE>_<REGISTER>_<FIELD>(<NUMBER>);
    //
    // For example, the following three lines of code are equivalent methods of
    // writing the value for 12MHZ to the CLKSEL field in the ADC_CFG register.
    //
    AM_REG(ADC, CFG) |= AM_REG_ADC_CFG_CLKSEL_12MHZ;
    AM_REGn(ADC, 0, CFG) |= AM_REG_ADC_CFG_CLKSEL_12MHZ;
    AM_REG(ADC, CFG) |= AM_REG_ADC_CFG_CLKSEL(0x1);

### Register Fields:

31 | 30 | 29 | 28 | 27 | 26 | 25 | 24 | 23 | 22 | 21 | 20 | 19 | 18 | 17 | 16 | 15 | 14 | 13 | 12 | 11 | 10 | 9 | 8 | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0
--- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | ---
RSVD 0x0 | ADCCALIBRATED 0x0 | CALONPWRUP 0x1

Bits | Name | RW | Description
--- | --- | --- | ---
31:2 | RSVD | RO | RESERVED.
1 | ADCCALIBRATED | RO | Status for ADC Calibration FALSE = 0x0 - ADC is not calibrated TRUE = 0x1 - ADC is calibrated
0 | CALONPWRUP | RW | Run ADC Calibration on initial power up sequence DIS = 0x0 - Disable automatic calibration on initial power up EN = 0x1 - Enable automatic calibration on initial power up

### ADCBATTLOAD - ADC Battery Load Enable

### Address:

Instance 0 Address: | 0x40020110

### Description:

ADC Battery Load Enable

### Example Macro Usage:

    //
    // All macro-based register writes follow the same basic format. For
    // single-instance modules, you may use the simpler AM_REG macro. For
    // multi-instance macros, you will need to specify the instance number using
    // the AM_REGn macro format.
    //
    // AM_REG(<MODULE>, <REGISTER>) |= AM_REG_<MODULE>_<REGISTER>_<FIELD>_<VALUE>;
    // AM_REGn(<MODULE>, <INSTANCE>, <REGISTER>) |= AM_REG_<MODULE>_<REGISTER>_<FIELD>_<VALUE>;
    //
    // For registers that do not have specific enumeration values, you may use this alternate format instead.
    //
    // AM_REG(<MODULE>, <REGISTER>) |= AM_REG_<MODULE>_<REGISTER>_<FIELD>(<NUMBER>);
    //
    // For example, the following three lines of code are equivalent methods of
    // writing the value for 12MHZ to the CLKSEL field in the ADC_CFG register.
    //
    AM_REG(ADC, CFG) |= AM_REG_ADC_CFG_CLKSEL_12MHZ;
    AM_REGn(ADC, 0, CFG) |= AM_REG_ADC_CFG_CLKSEL_12MHZ;
    AM_REG(ADC, CFG) |= AM_REG_ADC_CFG_CLKSEL(0x1);

### Register Fields:

31 | 30 | 29 | 28 | 27 | 26 | 25 | 24 | 23 | 22 | 21 | 20 | 19 | 18 | 17 | 16 | 15 | 14 | 13 | 12 | 11 | 10 | 9 | 8 | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0
--- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | ---
RSVD 0x0 | BATTLOAD 0x0

Bits | Name | RW | Description
--- | --- | --- | ---
31:1 | RSVD | RO | RESERVED.
0 | BATTLOAD | RW | Enable the ADC battery load resistor DIS = 0x0 - Battery load is disconnected EN = 0x1 - Battery load is enabled

### ADCREFCOMP - ADC Referece Keeper and Comparator Control

### Address:

Instance 0 Address: | 0x4002011C

### Description:

ADC Referece Keeper and Comparator Control

### Example Macro Usage:

    //
    // All macro-based register writes follow the same basic format. For
    // single-instance modules, you may use the simpler AM_REG macro. For
    // multi-instance macros, you will need to specify the instance number using
    // the AM_REGn macro format.
    //
    // AM_REG(<MODULE>, <REGISTER>) |= AM_REG_<MODULE>_<REGISTER>_<FIELD>_<VALUE>;
    // AM_REGn(<MODULE>, <INSTANCE>, <REGISTER>) |= AM_REG_<MODULE>_<REGISTER>_<FIELD>_<VALUE>;
    //
    // For registers that do not have specific enumeration values, you may use this alternate format instead.
    //
    // AM_REG(<MODULE>, <REGISTER>) |= AM_REG_<MODULE>_<REGISTER>_<FIELD>(<NUMBER>);
    //
    // For example, the following three lines of code are equivalent methods of
    // writing the value for 12MHZ to the CLKSEL field in the ADC_CFG register.
    //
    AM_REG(ADC, CFG) |= AM_REG_ADC_CFG_CLKSEL_12MHZ;
    AM_REGn(ADC, 0, CFG) |= AM_REG_ADC_CFG_CLKSEL_12MHZ;
    AM_REG(ADC, CFG) |= AM_REG_ADC_CFG_CLKSEL(0x1);

### Register Fields:

31 | 30 | 29 | 28 | 27 | 26 | 25 | 24 | 23 | 22 | 21 | 20 | 19 | 18 | 17 | 16 | 15 | 14 | 13 | 12 | 11 | 10 | 9 | 8 | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0
--- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | ---
RSVD 0x0 | ADCRFCMPEN 0x0 | RSVD 0x0 | ADCREFKEEPTRIM 0x0 | RSVD 0x0 | ADC_REFCOMP_OUT 0x0

Bits | Name | RW | Description
--- | --- | --- | ---
31:17 | RSVD | RO | RESERVED
16 | ADCRFCMPEN | RW | ADC Reference comparator power down
15:13 | RSVD | RO | RESERVED
12:8 | ADCREFKEEPTRIM | RW | ADC Reference Keeper Trim
7:1 | RSVD | RO | RESERVED
0 | ADC_REFCOMP_OUT | RO | Output of the ADC reference comparator

### XTALGENCTRL - XTAL Oscillator General Control

### Address:

Instance 0 Address: | 0x40020124

### Description:

XTAL Oscillator General Control

### Example Macro Usage:

    //
    // All macro-based register writes follow the same basic format. For
    // single-instance modules, you may use the simpler AM_REG macro. For
    // multi-instance macros, you will need to specify the instance number using
    // the AM_REGn macro format.
    //
    // AM_REG(<MODULE>, <REGISTER>) |= AM_REG_<MODULE>_<REGISTER>_<FIELD>_<VALUE>;
    // AM_REGn(<MODULE>, <INSTANCE>, <REGISTER>) |= AM_REG_<MODULE>_<REGISTER>_<FIELD>_<VALUE>;
    //
    // For registers that do not have specific enumeration values, you may use this alternate format instead.
    //
    // AM_REG(<MODULE>, <REGISTER>) |= AM_REG_<MODULE>_<REGISTER>_<FIELD>(<NUMBER>);
    //
    // For example, the following three lines of code are equivalent methods of
    // writing the value for 12MHZ to the CLKSEL field in the ADC_CFG register.
    //
    AM_REG(ADC, CFG) |= AM_REG_ADC_CFG_CLKSEL_12MHZ;
    AM_REGn(ADC, 0, CFG) |= AM_REG_ADC_CFG_CLKSEL_12MHZ;
    AM_REG(ADC, CFG) |= AM_REG_ADC_CFG_CLKSEL(0x1);

### Register Fields:

31 | 30 | 29 | 28 | 27 | 26 | 25 | 24 | 23 | 22 | 21 | 20 | 19 | 18 | 17 | 16 | 15 | 14 | 13 | 12 | 11 | 10 | 9 | 8 | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0
--- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | ---
RSVD 0x0 | XTALKSBIASTRIM 0x0 | XTALBIASTRIM 0x0 | ACWARMUP 0x0

Bits | Name | RW | Description
--- | --- | --- | ---
31:14 | RSVD | RO | RESERVED.
13:8 | XTALKSBIASTRIM | RW | XTAL IBIAS Kick start trim . This trim value is used during the startup prcess to enable a faster lock
7:2 | XTALBIASTRIM | RW | XTAL IBIAS trim
1:0 | ACWARMUP | RW | Auto-calibration delay control 1SEC = 0x0 - Warmup period of 1-2 seconds 2SEC = 0x1 - Warmup period of 2-4 seconds 4SEC = 0x2 - Warmup period of 4-8 seconds 8SEC = 0x3 - Warmup period of 8-16 seconds

### BOOTLOADERLOW - Determines whether the bootloader code is visible at address 0x00000000

### Address:

Instance 0 Address: | 0x400201A0

### Description:

Determines whether the bootloader code is visible at address 0x00000000

### Example Macro Usage:

    //
    // All macro-based register writes follow the same basic format. For
    // single-instance modules, you may use the simpler AM_REG macro. For
    // multi-instance macros, you will need to specify the instance number using
    // the AM_REGn macro format.
    //
    // AM_REG(<MODULE>, <REGISTER>) |= AM_REG_<MODULE>_<REGISTER>_<FIELD>_<VALUE>;
    // AM_REGn(<MODULE>, <INSTANCE>, <REGISTER>) |= AM_REG_<MODULE>_<REGISTER>_<FIELD>_<VALUE>;
    //
    // For registers that do not have specific enumeration values, you may use this alternate format instead.
    //
    // AM_REG(<MODULE>, <REGISTER>) |= AM_REG_<MODULE>_<REGISTER>_<FIELD>(<NUMBER>);
    //
    // For example, the following three lines of code are equivalent methods of
    // writing the value for 12MHZ to the CLKSEL field in the ADC_CFG register.
    //
    AM_REG(ADC, CFG) |= AM_REG_ADC_CFG_CLKSEL_12MHZ;
    AM_REGn(ADC, 0, CFG) |= AM_REG_ADC_CFG_CLKSEL_12MHZ;
    AM_REG(ADC, CFG) |= AM_REG_ADC_CFG_CLKSEL(0x1);

### Register Fields:

31 | 30 | 29 | 28 | 27 | 26 | 25 | 24 | 23 | 22 | 21 | 20 | 19 | 18 | 17 | 16 | 15 | 14 | 13 | 12 | 11 | 10 | 9 | 8 | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0
--- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | ---
RSVD 0x0 | VALUE 0x1

Bits | Name | RW | Description
--- | --- | --- | ---
31:1 | RSVD | RO | RESERVED.
0 | VALUE | RW | Determines whether the bootloader code is visible at address 0x00000000 or not. ADDR0 = 0x1 - Bootloader code at 0x00000000.

### SHADOWVALID - Register to indicate whether the shadow registers have been successfully loaded from the Flash Information Space.

### Address:

Instance 0 Address: | 0x400201A4

### Description:

Register to indicate whether the shadow registers have been successfully loaded from the Flash Information Space.

### Example Macro Usage:

    //
    // All macro-based register writes follow the same basic format. For
    // single-instance modules, you may use the simpler AM_REG macro. For
    // multi-instance macros, you will need to specify the instance number using
    // the AM_REGn macro format.
    //
    // AM_REG(<MODULE>, <REGISTER>) |= AM_REG_<MODULE>_<REGISTER>_<FIELD>_<VALUE>;
    // AM_REGn(<MODULE>, <INSTANCE>, <REGISTER>) |= AM_REG_<MODULE>_<REGISTER>_<FIELD>_<VALUE>;
    //
    // For registers that do not have specific enumeration values, you may use this alternate format instead.
    //
    // AM_REG(<MODULE>, <REGISTER>) |= AM_REG_<MODULE>_<REGISTER>_<FIELD>(<NUMBER>);
    //
    // For example, the following three lines of code are equivalent methods of
    // writing the value for 12MHZ to the CLKSEL field in the ADC_CFG register.
    //
    AM_REG(ADC, CFG) |= AM_REG_ADC_CFG_CLKSEL_12MHZ;
    AM_REGn(ADC, 0, CFG) |= AM_REG_ADC_CFG_CLKSEL_12MHZ;
    AM_REG(ADC, CFG) |= AM_REG_ADC_CFG_CLKSEL(0x1);

### Register Fields:

31 | 30 | 29 | 28 | 27 | 26 | 25 | 24 | 23 | 22 | 21 | 20 | 19 | 18 | 17 | 16 | 15 | 14 | 13 | 12 | 11 | 10 | 9 | 8 | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0
--- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | ---
RSVD 0x0 | BL_DSLEEP 0x1 | VALID 0x1

Bits | Name | RW | Description
--- | --- | --- | ---
31:2 | RSVD | RO | RESERVED.
1 | BL_DSLEEP | RO | Indicates whether the bootloader should sleep or deep sleep if no image loaded. DEEPSLEEP = 0x1 - Bootloader will go to deep sleep if no flash image loaded
0 | VALID | RO | Indicates whether the shadow registers contain valid data from the Flash Information Space. VALID = 0x1 - Flash information space contains valid data.

### ICODEFAULTADDR - ICODE bus address which was present when a bus fault occurred.

### Address:

Instance 0 Address: | 0x400201C0

### Description:

ICODE bus address which was present when a bus fault occurred.

### Example Macro Usage:

    //
    // All macro-based register writes follow the same basic format. For
    // single-instance modules, you may use the simpler AM_REG macro. For
    // multi-instance macros, you will need to specify the instance number using
    // the AM_REGn macro format.
    //
    // AM_REG(<MODULE>, <REGISTER>) |= AM_REG_<MODULE>_<REGISTER>_<FIELD>_<VALUE>;
    // AM_REGn(<MODULE>, <INSTANCE>, <REGISTER>) |= AM_REG_<MODULE>_<REGISTER>_<FIELD>_<VALUE>;
    //
    // For registers that do not have specific enumeration values, you may use this alternate format instead.
    //
    // AM_REG(<MODULE>, <REGISTER>) |= AM_REG_<MODULE>_<REGISTER>_<FIELD>(<NUMBER>);
    //
    // For example, the following three lines of code are equivalent methods of
    // writing the value for 12MHZ to the CLKSEL field in the ADC_CFG register.
    //
    AM_REG(ADC, CFG) |= AM_REG_ADC_CFG_CLKSEL_12MHZ;
    AM_REGn(ADC, 0, CFG) |= AM_REG_ADC_CFG_CLKSEL_12MHZ;
    AM_REG(ADC, CFG) |= AM_REG_ADC_CFG_CLKSEL(0x1);

### Register Fields:

31 | 30 | 29 | 28 | 27 | 26 | 25 | 24 | 23 | 22 | 21 | 20 | 19 | 18 | 17 | 16 | 15 | 14 | 13 | 12 | 11 | 10 | 9 | 8 | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0
--- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | ---
ADDR 0x0

Bits | Name | RW | Description
--- | --- | --- | ---
31:0 | ADDR | RO | The ICODE bus address observed when a Bus Fault occurred. Once an address is captured in this field, it is held until the corresponding Fault Observed bit is cleared in the FAULTSTATUS register.

### DCODEFAULTADDR - DCODE bus address which was present when a bus fault occurred.

### Address:

Instance 0 Address: | 0x400201C4

### Description:

DCODE bus address which was present when a bus fault occurred.

### Example Macro Usage:

    //
    // All macro-based register writes follow the same basic format. For
    // single-instance modules, you may use the simpler AM_REG macro. For
    // multi-instance macros, you will need to specify the instance number using
    // the AM_REGn macro format.
    //
    // AM_REG(<MODULE>, <REGISTER>) |= AM_REG_<MODULE>_<REGISTER>_<FIELD>_<VALUE>;
    // AM_REGn(<MODULE>, <INSTANCE>, <REGISTER>) |= AM_REG_<MODULE>_<REGISTER>_<FIELD>_<VALUE>;
    //
    // For registers that do not have specific enumeration values, you may use this alternate format instead.
    //
    // AM_REG(<MODULE>, <REGISTER>) |= AM_REG_<MODULE>_<REGISTER>_<FIELD>(<NUMBER>);
    //
    // For example, the following three lines of code are equivalent methods of
    // writing the value for 12MHZ to the CLKSEL field in the ADC_CFG register.
    //
    AM_REG(ADC, CFG) |= AM_REG_ADC_CFG_CLKSEL_12MHZ;
    AM_REGn(ADC, 0, CFG) |= AM_REG_ADC_CFG_CLKSEL_12MHZ;
    AM_REG(ADC, CFG) |= AM_REG_ADC_CFG_CLKSEL(0x1);

### Register Fields:

31 | 30 | 29 | 28 | 27 | 26 | 25 | 24 | 23 | 22 | 21 | 20 | 19 | 18 | 17 | 16 | 15 | 14 | 13 | 12 | 11 | 10 | 9 | 8 | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0
--- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | ---
ADDR 0x0

Bits | Name | RW | Description
--- | --- | --- | ---
31:0 | ADDR | RO | The DCODE bus address observed when a Bus Fault occurred. Once an address is captured in this field, it is held until the corresponding Fault Observed bit is cleared in the FAULTSTATUS register.

### SYSFAULTADDR - System bus address which was present when a bus fault occurred.

### Address:

Instance 0 Address: | 0x400201C8

### Description:

System bus address which was present when a bus fault occurred.

### Example Macro Usage:

    //
    // All macro-based register writes follow the same basic format. For
    // single-instance modules, you may use the simpler AM_REG macro. For
    // multi-instance macros, you will need to specify the instance number using
    // the AM_REGn macro format.
    //
    // AM_REG(<MODULE>, <REGISTER>) |= AM_REG_<MODULE>_<REGISTER>_<FIELD>_<VALUE>;
    // AM_REGn(<MODULE>, <INSTANCE>, <REGISTER>) |= AM_REG_<MODULE>_<REGISTER>_<FIELD>_<VALUE>;
    //
    // For registers that do not have specific enumeration values, you may use this alternate format instead.
    //
    // AM_REG(<MODULE>, <REGISTER>) |= AM_REG_<MODULE>_<REGISTER>_<FIELD>(<NUMBER>);
    //
    // For example, the following three lines of code are equivalent methods of
    // writing the value for 12MHZ to the CLKSEL field in the ADC_CFG register.
    //
    AM_REG(ADC, CFG) |= AM_REG_ADC_CFG_CLKSEL_12MHZ;
    AM_REGn(ADC, 0, CFG) |= AM_REG_ADC_CFG_CLKSEL_12MHZ;
    AM_REG(ADC, CFG) |= AM_REG_ADC_CFG_CLKSEL(0x1);

### Register Fields:

31 | 30 | 29 | 28 | 27 | 26 | 25 | 24 | 23 | 22 | 21 | 20 | 19 | 18 | 17 | 16 | 15 | 14 | 13 | 12 | 11 | 10 | 9 | 8 | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0
--- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | ---
ADDR 0x0

Bits | Name | RW | Description
--- | --- | --- | ---
31:0 | ADDR | RO | SYS bus address observed when a Bus Fault occurred. Once an address is captured in this field, it is held until the corresponding Fault Observed bit is cleared in the FAULTSTATUS register.

### FAULTSTATUS - Reflects the status of the bus decoders' fault detection. Any write to this register will clear all of the status bits within the register.

### Address:

Instance 0 Address: | 0x400201CC

### Description:

Reflects the status of the bus decoders' fault detection. Any write to this register will clear all of the status bits within the register.

### Example Macro Usage:

    //
    // All macro-based register writes follow the same basic format. For
    // single-instance modules, you may use the simpler AM_REG macro. For
    // multi-instance macros, you will need to specify the instance number using
    // the AM_REGn macro format.
    //
    // AM_REG(<MODULE>, <REGISTER>) |= AM_REG_<MODULE>_<REGISTER>_<FIELD>_<VALUE>;
    // AM_REGn(<MODULE>, <INSTANCE>, <REGISTER>) |= AM_REG_<MODULE>_<REGISTER>_<FIELD>_<VALUE>;
    //
    // For registers that do not have specific enumeration values, you may use this alternate format instead.
    //
    // AM_REG(<MODULE>, <REGISTER>) |= AM_REG_<MODULE>_<REGISTER>_<FIELD>(<NUMBER>);
    //
    // For example, the following three lines of code are equivalent methods of
    // writing the value for 12MHZ to the CLKSEL field in the ADC_CFG register.
    //
    AM_REG(ADC, CFG) |= AM_REG_ADC_CFG_CLKSEL_12MHZ;
    AM_REGn(ADC, 0, CFG) |= AM_REG_ADC_CFG_CLKSEL_12MHZ;
    AM_REG(ADC, CFG) |= AM_REG_ADC_CFG_CLKSEL(0x1);

### Register Fields:

31 | 30 | 29 | 28 | 27 | 26 | 25 | 24 | 23 | 22 | 21 | 20 | 19 | 18 | 17 | 16 | 15 | 14 | 13 | 12 | 11 | 10 | 9 | 8 | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0
--- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | ---
RSVD 0x0 | SYS 0x0 | DCODE 0x0 | ICODE 0x0

Bits | Name | RW | Description
--- | --- | --- | ---
31:3 | RSVD | RO | RESERVED.
2 | SYS | RW | SYS Bus Decoder Fault Detected bit. When set, a fault has been detected, and the SYSFAULTADDR register will contain the bus address which generated the fault. NOFAULT = 0x0 - No bus fault has been detected. FAULT = 0x1 - Bus fault detected.
1 | DCODE | RW | DCODE Bus Decoder Fault Detected bit. When set, a fault has been detected, and the DCODEFAULTADDR register will contain the bus address which generated the fault. NOFAULT = 0x0 - No DCODE fault has been detected. FAULT = 0x1 - DCODE fault detected.
0 | ICODE | RW | The ICODE Bus Decoder Fault Detected bit. When set, a fault has been detected, and the ICODEFAULTADDR register will contain the bus address which generated the fault. NOFAULT = 0x0 - No ICODE fault has been detected. FAULT = 0x1 - ICODE fault detected.

### FAULTCAPTUREEN - Enable the fault capture registers

### Address:

Instance 0 Address: | 0x400201D0

### Description:

Enable the fault capture registers

### Example Macro Usage:

    //
    // All macro-based register writes follow the same basic format. For
    // single-instance modules, you may use the simpler AM_REG macro. For
    // multi-instance macros, you will need to specify the instance number using
    // the AM_REGn macro format.
    //
    // AM_REG(<MODULE>, <REGISTER>) |= AM_REG_<MODULE>_<REGISTER>_<FIELD>_<VALUE>;
    // AM_REGn(<MODULE>, <INSTANCE>, <REGISTER>) |= AM_REG_<MODULE>_<REGISTER>_<FIELD>_<VALUE>;
    //
    // For registers that do not have specific enumeration values, you may use this alternate format instead.
    //
    // AM_REG(<MODULE>, <REGISTER>) |= AM_REG_<MODULE>_<REGISTER>_<FIELD>(<NUMBER>);
    //
    // For example, the following three lines of code are equivalent methods of
    // writing the value for 12MHZ to the CLKSEL field in the ADC_CFG register.
    //
    AM_REG(ADC, CFG) |= AM_REG_ADC_CFG_CLKSEL_12MHZ;
    AM_REGn(ADC, 0, CFG) |= AM_REG_ADC_CFG_CLKSEL_12MHZ;
    AM_REG(ADC, CFG) |= AM_REG_ADC_CFG_CLKSEL(0x1);

### Register Fields:

31 | 30 | 29 | 28 | 27 | 26 | 25 | 24 | 23 | 22 | 21 | 20 | 19 | 18 | 17 | 16 | 15 | 14 | 13 | 12 | 11 | 10 | 9 | 8 | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0
--- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | ---
RSVD 0x0 | ENABLE 0x0

Bits | Name | RW | Description
--- | --- | --- | ---
31:1 | RSVD | RO | RESERVED.
0 | ENABLE | RW | Fault Capture Enable field. When set, the Fault Capture monitors are enabled and addresses which generate a hard fault are captured into the FAULTADDR registers. DIS = 0x0 - Disable fault capture. EN = 0x1 - Enable fault capture.

### DBGR1 - Read-only debug register 1

### Address:

Instance 0 Address: | 0x40020200

### Description:

Read-only debug register 1

### Example Macro Usage:

    //
    // All macro-based register writes follow the same basic format. For
    // single-instance modules, you may use the simpler AM_REG macro. For
    // multi-instance macros, you will need to specify the instance number using
    // the AM_REGn macro format.
    //
    // AM_REG(<MODULE>, <REGISTER>) |= AM_REG_<MODULE>_<REGISTER>_<FIELD>_<VALUE>;
    // AM_REGn(<MODULE>, <INSTANCE>, <REGISTER>) |= AM_REG_<MODULE>_<REGISTER>_<FIELD>_<VALUE>;
    //
    // For registers that do not have specific enumeration values, you may use this alternate format instead.
    //
    // AM_REG(<MODULE>, <REGISTER>) |= AM_REG_<MODULE>_<REGISTER>_<FIELD>(<NUMBER>);
    //
    // For example, the following three lines of code are equivalent methods of
    // writing the value for 12MHZ to the CLKSEL field in the ADC_CFG register.
    //
    AM_REG(ADC, CFG) |= AM_REG_ADC_CFG_CLKSEL_12MHZ;
    AM_REGn(ADC, 0, CFG) |= AM_REG_ADC_CFG_CLKSEL_12MHZ;
    AM_REG(ADC, CFG) |= AM_REG_ADC_CFG_CLKSEL(0x1);

### Register Fields:

31 | 30 | 29 | 28 | 27 | 26 | 25 | 24 | 23 | 22 | 21 | 20 | 19 | 18 | 17 | 16 | 15 | 14 | 13 | 12 | 11 | 10 | 9 | 8 | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0
--- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | ---
ONETO8 0x12345678

Bits | Name | RW | Description
--- | --- | --- | ---
31:0 | ONETO8 | RO | Read-only register for communication validation

### DBGR2 - Read-only debug register 2

### Address:

Instance 0 Address: | 0x40020204

### Description:

Read-only debug register 2

### Example Macro Usage:

    //
    // All macro-based register writes follow the same basic format. For
    // single-instance modules, you may use the simpler AM_REG macro. For
    // multi-instance macros, you will need to specify the instance number using
    // the AM_REGn macro format.
    //
    // AM_REG(<MODULE>, <REGISTER>) |= AM_REG_<MODULE>_<REGISTER>_<FIELD>_<VALUE>;
    // AM_REGn(<MODULE>, <INSTANCE>, <REGISTER>) |= AM_REG_<MODULE>_<REGISTER>_<FIELD>_<VALUE>;
    //
    // For registers that do not have specific enumeration values, you may use this alternate format instead.
    //
    // AM_REG(<MODULE>, <REGISTER>) |= AM_REG_<MODULE>_<REGISTER>_<FIELD>(<NUMBER>);
    //
    // For example, the following three lines of code are equivalent methods of
    // writing the value for 12MHZ to the CLKSEL field in the ADC_CFG register.
    //
    AM_REG(ADC, CFG) |= AM_REG_ADC_CFG_CLKSEL_12MHZ;
    AM_REGn(ADC, 0, CFG) |= AM_REG_ADC_CFG_CLKSEL_12MHZ;
    AM_REG(ADC, CFG) |= AM_REG_ADC_CFG_CLKSEL(0x1);

### Register Fields:

31 | 30 | 29 | 28 | 27 | 26 | 25 | 24 | 23 | 22 | 21 | 20 | 19 | 18 | 17 | 16 | 15 | 14 | 13 | 12 | 11 | 10 | 9 | 8 | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0
--- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | ---
COOLCODE 0xc001c0de

Bits | Name | RW | Description
--- | --- | --- | ---
31:0 | COOLCODE | RO | Read-only register for communication validation

### PMUENABLE - Control bit to enable/disable the PMU

### Address:

Instance 0 Address: | 0x40020220

### Description:

Control bit to enable/disable the PMU

### Example Macro Usage:

    //
    // All macro-based register writes follow the same basic format. For
    // single-instance modules, you may use the simpler AM_REG macro. For
    // multi-instance macros, you will need to specify the instance number using
    // the AM_REGn macro format.
    //
    // AM_REG(<MODULE>, <REGISTER>) |= AM_REG_<MODULE>_<REGISTER>_<FIELD>_<VALUE>;
    // AM_REGn(<MODULE>, <INSTANCE>, <REGISTER>) |= AM_REG_<MODULE>_<REGISTER>_<FIELD>_<VALUE>;
    //
    // For registers that do not have specific enumeration values, you may use this alternate format instead.
    //
    // AM_REG(<MODULE>, <REGISTER>) |= AM_REG_<MODULE>_<REGISTER>_<FIELD>(<NUMBER>);
    //
    // For example, the following three lines of code are equivalent methods of
    // writing the value for 12MHZ to the CLKSEL field in the ADC_CFG register.
    //
    AM_REG(ADC, CFG) |= AM_REG_ADC_CFG_CLKSEL_12MHZ;
    AM_REGn(ADC, 0, CFG) |= AM_REG_ADC_CFG_CLKSEL_12MHZ;
    AM_REG(ADC, CFG) |= AM_REG_ADC_CFG_CLKSEL(0x1);

### Register Fields:

31 | 30 | 29 | 28 | 27 | 26 | 25 | 24 | 23 | 22 | 21 | 20 | 19 | 18 | 17 | 16 | 15 | 14 | 13 | 12 | 11 | 10 | 9 | 8 | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0
--- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | ---
RSVD 0x0 | ENABLE 0x1

Bits | Name | RW | Description
--- | --- | --- | ---
31:1 | RSVD | RO | RESERVED.
0 | ENABLE | RW | PMU Enable Control bit. When set, the MCU's PMU will place the MCU into the lowest power consuming Deep Sleep mode upon execution of a WFI instruction (dependent on the setting of the SLEEPDEEP bit in the ARM SCR register). When cleared, regardless of the requested sleep mode, the PMU will not enter the lowest power Deep Sleep mode, instead entering the Sleep mode. DIS = 0x0 - Disable MCU power management. EN = 0x1 - Enable MCU power management.

### TPIUCTRL - TPIU Control Register. Determines the clock enable and frequency for the M4's TPIU interface.

### Address:

Instance 0 Address: | 0x40020250

### Description:

TPIU Control Register. Determines the clock enable and frequency for the M4's TPIU interface.

### Example Macro Usage:

    //
    // All macro-based register writes follow the same basic format. For
    // single-instance modules, you may use the simpler AM_REG macro. For
    // multi-instance macros, you will need to specify the instance number using
    // the AM_REGn macro format.
    //
    // AM_REG(<MODULE>, <REGISTER>) |= AM_REG_<MODULE>_<REGISTER>_<FIELD>_<VALUE>;
    // AM_REGn(<MODULE>, <INSTANCE>, <REGISTER>) |= AM_REG_<MODULE>_<REGISTER>_<FIELD>_<VALUE>;
    //
    // For registers that do not have specific enumeration values, you may use this alternate format instead.
    //
    // AM_REG(<MODULE>, <REGISTER>) |= AM_REG_<MODULE>_<REGISTER>_<FIELD>(<NUMBER>);
    //
    // For example, the following three lines of code are equivalent methods of
    // writing the value for 12MHZ to the CLKSEL field in the ADC_CFG register.
    //
    AM_REG(ADC, CFG) |= AM_REG_ADC_CFG_CLKSEL_12MHZ;
    AM_REGn(ADC, 0, CFG) |= AM_REG_ADC_CFG_CLKSEL_12MHZ;
    AM_REG(ADC, CFG) |= AM_REG_ADC_CFG_CLKSEL(0x1);

### Register Fields:

31 | 30 | 29 | 28 | 27 | 26 | 25 | 24 | 23 | 22 | 21 | 20 | 19 | 18 | 17 | 16 | 15 | 14 | 13 | 12 | 11 | 10 | 9 | 8 | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0
--- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | ---
RSVD 0x0 | CLKSEL 0x0 | RSVD 0x0 | ENABLE 0x0

Bits | Name | RW | Description
--- | --- | --- | ---
31:11 | RSVD | RO | RESERVED.
10:8 | CLKSEL | RW | This field selects the frequency of the ARM M4 TPIU port. LOW_PWR = 0x0 - Low power state. 0MHz = 0x0 - Low power state. 24MHZ = 0x1 - Selects 6MHz frequency. 6MHZ = 0x2 - Selects 6MHz frequency. 3MHZ = 0x3 - Selects 3MHz frequency. 1_5MHZ = 0x4 - Selects 1.5 MHz frequency.
7:1 | RSVD | RO | RESERVED.
0 | ENABLE | RW | TPIU Enable field. When set, the ARM M4 TPIU is enabled and data can be streamed out of the MCU's SWO port using the ARM ITM and TPIU modules. DIS = 0x0 - Disable the TPIU. EN = 0x1 - Enable the TPIU.

### KEXTCLKSEL - Key Register to enable the use of external clock selects via the EXTCLKSEL reg

### Address:

Instance 0 Address: | 0x40020348

### Description:

Key Register to enable the use of external clock selects via the EXTCLKSEL reg

### Example Macro Usage:

    //
    // All macro-based register writes follow the same basic format. For
    // single-instance modules, you may use the simpler AM_REG macro. For
    // multi-instance macros, you will need to specify the instance number using
    // the AM_REGn macro format.
    //
    // AM_REG(<MODULE>, <REGISTER>) |= AM_REG_<MODULE>_<REGISTER>_<FIELD>_<VALUE>;
    // AM_REGn(<MODULE>, <INSTANCE>, <REGISTER>) |= AM_REG_<MODULE>_<REGISTER>_<FIELD>_<VALUE>;
    //
    // For registers that do not have specific enumeration values, you may use this alternate format instead.
    //
    // AM_REG(<MODULE>, <REGISTER>) |= AM_REG_<MODULE>_<REGISTER>_<FIELD>(<NUMBER>);
    //
    // For example, the following three lines of code are equivalent methods of
    // writing the value for 12MHZ to the CLKSEL field in the ADC_CFG register.
    //
    AM_REG(ADC, CFG) |= AM_REG_ADC_CFG_CLKSEL_12MHZ;
    AM_REGn(ADC, 0, CFG) |= AM_REG_ADC_CFG_CLKSEL_12MHZ;
    AM_REG(ADC, CFG) |= AM_REG_ADC_CFG_CLKSEL(0x1);

### Register Fields:

31 | 30 | 29 | 28 | 27 | 26 | 25 | 24 | 23 | 22 | 21 | 20 | 19 | 18 | 17 | 16 | 15 | 14 | 13 | 12 | 11 | 10 | 9 | 8 | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0
--- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | ---
KEXTCLKSEL 0x0

Bits | Name | RW | Description
--- | --- | --- | ---
31:0 | KEXTCLKSEL | RW | Key register value. Key = 0x53 - Key