Name:
=====
 adc_lpmode2


Description:
============
 Example that takes samples with the ADC at 1Hz and powers off the

ADC between samples.  CTIMER-A1 is used to drive the process.

SWO is configured in 1M baud, 8-n-1 mode.


******************************************************************************


