Name:
=====
 adc_lpmode1


Description:
============
 Example that periodically takes samples with the ADC.


This example shows the CTIMER-A3 triggering repeated samples of the
temperature sensor in low-power mode 1.

SWO is configured in 1M baud, 8-n-1 mode.


******************************************************************************


