| Apollo Register Documentation v2.2.0

- Main Page

TPIU - ARM Trace Port Interface Unit

### TPIU Register Index

0xE0040000: | SSPSR - Supported Parallel Port Sizes.
0xE0040004: | CSPSR - Current Parallel Port Size.
0xE0040010: | ACPR - Asynchronous Clock Prescaler.
0xE00400F0: | SPPR - Selected Pin Protocol.
0xE0040304: | FFCR - Formatter and Flush Control Register.
0xE0040F00: | ITCTRL - Specifies normal or integration mode for the TPIU.
0xE0040FC8: | TYPE - TPIU Type.

### SSPSR - Supported Parallel Port Sizes.

### Address:

Instance 0 Address: | 0xE0040000

### Description:

Supported Parallel Port Sizes.

### Example Macro Usage:

    //
    // All macro-based register writes follow the same basic format. For
    // single-instance modules, you may use the simpler AM_REG macro. For
    // multi-instance macros, you will need to specify the instance number using
    // the AM_REGn macro format.
    //
    // AM_REG(<MODULE>, <REGISTER>) |= AM_REG_<MODULE>_<REGISTER>_<FIELD>_<VALUE>;
    // AM_REGn(<MODULE>, <INSTANCE>, <REGISTER>) |= AM_REG_<MODULE>_<REGISTER>_<FIELD>_<VALUE>;
    //
    // For registers that do not have specific enumeration values, you may use this alternate format instead.
    //
    // AM_REG(<MODULE>, <REGISTER>) |= AM_REG_<MODULE>_<REGISTER>_<FIELD>(<NUMBER>);
    //
    // For example, the following three lines of code are equivalent methods of
    // writing the value for 12MHZ to the CLKSEL field in the ADC_CFG register.
    //
    AM_REG(ADC, CFG) |= AM_REG_ADC_CFG_CLKSEL_12MHZ;
    AM_REGn(ADC, 0, CFG) |= AM_REG_ADC_CFG_CLKSEL_12MHZ;
    AM_REG(ADC, CFG) |= AM_REG_ADC_CFG_CLKSEL(0x1);

### Register Fields:

31 | 30 | 29 | 28 | 27 | 26 | 25 | 24 | 23 | 22 | 21 | 20 | 19 | 18 | 17 | 16 | 15 | 14 | 13 | 12 | 11 | 10 | 9 | 8 | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0
--- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | ---
SWIDTH0 0x1

Bits | Name | RW | Description
--- | --- | --- | ---
0 | SWIDTH0 | RO | Parallel Port Width 1 supported

### CSPSR - Current Parallel Port Size.

### Address:

Instance 0 Address: | 0xE0040004

### Description:

Current Parallel Port Size.

### Example Macro Usage:

    //
    // All macro-based register writes follow the same basic format. For
    // single-instance modules, you may use the simpler AM_REG macro. For
    // multi-instance macros, you will need to specify the instance number using
    // the AM_REGn macro format.
    //
    // AM_REG(<MODULE>, <REGISTER>) |= AM_REG_<MODULE>_<REGISTER>_<FIELD>_<VALUE>;
    // AM_REGn(<MODULE>, <INSTANCE>, <REGISTER>) |= AM_REG_<MODULE>_<REGISTER>_<FIELD>_<VALUE>;
    //
    // For registers that do not have specific enumeration values, you may use this alternate format instead.
    //
    // AM_REG(<MODULE>, <REGISTER>) |= AM_REG_<MODULE>_<REGISTER>_<FIELD>(<NUMBER>);
    //
    // For example, the following three lines of code are equivalent methods of
    // writing the value for 12MHZ to the CLKSEL field in the ADC_CFG register.
    //
    AM_REG(ADC, CFG) |= AM_REG_ADC_CFG_CLKSEL_12MHZ;
    AM_REGn(ADC, 0, CFG) |= AM_REG_ADC_CFG_CLKSEL_12MHZ;
    AM_REG(ADC, CFG) |= AM_REG_ADC_CFG_CLKSEL(0x1);

### Register Fields:

31 | 30 | 29 | 28 | 27 | 26 | 25 | 24 | 23 | 22 | 21 | 20 | 19 | 18 | 17 | 16 | 15 | 14 | 13 | 12 | 11 | 10 | 9 | 8 | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0
--- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | ---
CWIDTH 0x1

Bits | Name | RW | Description
--- | --- | --- | ---
31:0 | CWIDTH | RW | One-hot representation of the current port width. 1BIT = 0x1 - Set width to 1.

### ACPR - Asynchronous Clock Prescaler.

### Address:

Instance 0 Address: | 0xE0040010

### Description:

Asynchronous Clock Prescaler.

### Example Macro Usage:

    //
    // All macro-based register writes follow the same basic format. For
    // single-instance modules, you may use the simpler AM_REG macro. For
    // multi-instance macros, you will need to specify the instance number using
    // the AM_REGn macro format.
    //
    // AM_REG(<MODULE>, <REGISTER>) |= AM_REG_<MODULE>_<REGISTER>_<FIELD>_<VALUE>;
    // AM_REGn(<MODULE>, <INSTANCE>, <REGISTER>) |= AM_REG_<MODULE>_<REGISTER>_<FIELD>_<VALUE>;
    //
    // For registers that do not have specific enumeration values, you may use this alternate format instead.
    //
    // AM_REG(<MODULE>, <REGISTER>) |= AM_REG_<MODULE>_<REGISTER>_<FIELD>(<NUMBER>);
    //
    // For example, the following three lines of code are equivalent methods of
    // writing the value for 12MHZ to the CLKSEL field in the ADC_CFG register.
    //
    AM_REG(ADC, CFG) |= AM_REG_ADC_CFG_CLKSEL_12MHZ;
    AM_REGn(ADC, 0, CFG) |= AM_REG_ADC_CFG_CLKSEL_12MHZ;
    AM_REG(ADC, CFG) |= AM_REG_ADC_CFG_CLKSEL(0x1);

### Register Fields:

31 | 30 | 29 | 28 | 27 | 26 | 25 | 24 | 23 | 22 | 21 | 20 | 19 | 18 | 17 | 16 | 15 | 14 | 13 | 12 | 11 | 10 | 9 | 8 | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0
--- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | ---
RSVD 0x0 | SWOSCALER 0x0

Bits | Name | RW | Description
--- | --- | --- | ---
31:16 | RSVD | RO | RESERVED
15:0 | SWOSCALER | RW | Prescaler value for the baudrate of SWO. 115200 = 0x33 - Set divisor correctly for 115200 baud.

### SPPR - Selected Pin Protocol.

### Address:

Instance 0 Address: | 0xE00400F0

### Description:

Selected Pin Protocol.

### Example Macro Usage:

    //
    // All macro-based register writes follow the same basic format. For
    // single-instance modules, you may use the simpler AM_REG macro. For
    // multi-instance macros, you will need to specify the instance number using
    // the AM_REGn macro format.
    //
    // AM_REG(<MODULE>, <REGISTER>) |= AM_REG_<MODULE>_<REGISTER>_<FIELD>_<VALUE>;
    // AM_REGn(<MODULE>, <INSTANCE>, <REGISTER>) |= AM_REG_<MODULE>_<REGISTER>_<FIELD>_<VALUE>;
    //
    // For registers that do not have specific enumeration values, you may use this alternate format instead.
    //
    // AM_REG(<MODULE>, <REGISTER>) |= AM_REG_<MODULE>_<REGISTER>_<FIELD>(<NUMBER>);
    //
    // For example, the following three lines of code are equivalent methods of
    // writing the value for 12MHZ to the CLKSEL field in the ADC_CFG register.
    //
    AM_REG(ADC, CFG) |= AM_REG_ADC_CFG_CLKSEL_12MHZ;
    AM_REGn(ADC, 0, CFG) |= AM_REG_ADC_CFG_CLKSEL_12MHZ;
    AM_REG(ADC, CFG) |= AM_REG_ADC_CFG_CLKSEL(0x1);

### Register Fields:

31 | 30 | 29 | 28 | 27 | 26 | 25 | 24 | 23 | 22 | 21 | 20 | 19 | 18 | 17 | 16 | 15 | 14 | 13 | 12 | 11 | 10 | 9 | 8 | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0
--- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | ---
RSVD 0x0 | TXMODE 0x0

Bits | Name | RW | Description
--- | --- | --- | ---
31:2 | RSVD | RO | RESERVED
1:0 | TXMODE | RW | Selects the protocol used for trace output. PARALLEL = 0x0 - Parallel trace port. MANCHESTER = 0x1 - Manchester encoded. NRZ = 0x2 - Non-return-to-zero encoding. UART = 0x2 - UART encoding.

### FFCR - Formatter and Flush Control Register.

### Address:

Instance 0 Address: | 0xE0040304

### Description:

Formatter and Flush Control Register.

### Example Macro Usage:

    //
    // All macro-based register writes follow the same basic format. For
    // single-instance modules, you may use the simpler AM_REG macro. For
    // multi-instance macros, you will need to specify the instance number using
    // the AM_REGn macro format.
    //
    // AM_REG(<MODULE>, <REGISTER>) |= AM_REG_<MODULE>_<REGISTER>_<FIELD>_<VALUE>;
    // AM_REGn(<MODULE>, <INSTANCE>, <REGISTER>) |= AM_REG_<MODULE>_<REGISTER>_<FIELD>_<VALUE>;
    //
    // For registers that do not have specific enumeration values, you may use this alternate format instead.
    //
    // AM_REG(<MODULE>, <REGISTER>) |= AM_REG_<MODULE>_<REGISTER>_<FIELD>(<NUMBER>);
    //
    // For example, the following three lines of code are equivalent methods of
    // writing the value for 12MHZ to the CLKSEL field in the ADC_CFG register.
    //
    AM_REG(ADC, CFG) |= AM_REG_ADC_CFG_CLKSEL_12MHZ;
    AM_REGn(ADC, 0, CFG) |= AM_REG_ADC_CFG_CLKSEL_12MHZ;
    AM_REG(ADC, CFG) |= AM_REG_ADC_CFG_CLKSEL(0x1);

### Register Fields:

31 | 30 | 29 | 28 | 27 | 26 | 25 | 24 | 23 | 22 | 21 | 20 | 19 | 18 | 17 | 16 | 15 | 14 | 13 | 12 | 11 | 10 | 9 | 8 | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0
--- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | ---
RSVD 0x1 | ENFCONT 0x0 | RSVD 0x0

Bits | Name | RW | Description
--- | --- | --- | ---
31:2 | RSVD | RO | RESERVED
1 | ENFCONT | RW | Enable continuous formatting.
0 | RSVD | RO | RESERVED

### ITCTRL - Specifies normal or integration mode for the TPIU.

### Address:

Instance 0 Address: | 0xE0040F00

### Description:

Specifies normal or integration mode for the TPIU.

### Example Macro Usage:

    //
    // All macro-based register writes follow the same basic format. For
    // single-instance modules, you may use the simpler AM_REG macro. For
    // multi-instance macros, you will need to specify the instance number using
    // the AM_REGn macro format.
    //
    // AM_REG(<MODULE>, <REGISTER>) |= AM_REG_<MODULE>_<REGISTER>_<FIELD>_<VALUE>;
    // AM_REGn(<MODULE>, <INSTANCE>, <REGISTER>) |= AM_REG_<MODULE>_<REGISTER>_<FIELD>_<VALUE>;
    //
    // For registers that do not have specific enumeration values, you may use this alternate format instead.
    //
    // AM_REG(<MODULE>, <REGISTER>) |= AM_REG_<MODULE>_<REGISTER>_<FIELD>(<NUMBER>);
    //
    // For example, the following three lines of code are equivalent methods of
    // writing the value for 12MHZ to the CLKSEL field in the ADC_CFG register.
    //
    AM_REG(ADC, CFG) |= AM_REG_ADC_CFG_CLKSEL_12MHZ;
    AM_REGn(ADC, 0, CFG) |= AM_REG_ADC_CFG_CLKSEL_12MHZ;
    AM_REG(ADC, CFG) |= AM_REG_ADC_CFG_CLKSEL(0x1);

### Register Fields:

31 | 30 | 29 | 28 | 27 | 26 | 25 | 24 | 23 | 22 | 21 | 20 | 19 | 18 | 17 | 16 | 15 | 14 | 13 | 12 | 11 | 10 | 9 | 8 | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0
--- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | ---
RSVD 0x0 | MODE 0x0

Bits | Name | RW | Description
--- | --- | --- | ---
30:1 | RSVD | RO | RESERVED
1:0 | MODE | RW | Specifies the current mode for the TPIU. NORMAL = 0x0 - Normal mode. TEST = 0x1 - Integration test mode. DATA_TEST = 0x2 - Integration data test mode.

### TYPE - TPIU Type.

### Address:

Instance 0 Address: | 0xE0040FC8

### Description:

TPIU Type.

### Example Macro Usage:

    //
    // All macro-based register writes follow the same basic format. For
    // single-instance modules, you may use the simpler AM_REG macro. For
    // multi-instance macros, you will need to specify the instance number using
    // the AM_REGn macro format.
    //
    // AM_REG(<MODULE>, <REGISTER>) |= AM_REG_<MODULE>_<REGISTER>_<FIELD>_<VALUE>;
    // AM_REGn(<MODULE>, <INSTANCE>, <REGISTER>) |= AM_REG_<MODULE>_<REGISTER>_<FIELD>_<VALUE>;
    //
    // For registers that do not have specific enumeration values, you may use this alternate format instead.
    //
    // AM_REG(<MODULE>, <REGISTER>) |= AM_REG_<MODULE>_<REGISTER>_<FIELD>(<NUMBER>);
    //
    // For example, the following three lines of code are equivalent methods of
    // writing the value for 12MHZ to the CLKSEL field in the ADC_CFG register.
    //
    AM_REG(ADC, CFG) |= AM_REG_ADC_CFG_CLKSEL_12MHZ;
    AM_REGn(ADC, 0, CFG) |= AM_REG_ADC_CFG_CLKSEL_12MHZ;
    AM_REG(ADC, CFG) |= AM_REG_ADC_CFG_CLKSEL(0x1);

### Register Fields:

31 | 30 | 29 | 28 | 27 | 26 | 25 | 24 | 23 | 22 | 21 | 20 | 19 | 18 | 17 | 16 | 15 | 14 | 13 | 12 | 11 | 10 | 9 | 8 | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0
--- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | ---
RSVD 0x0 | NRZVALID 0x1 | MANCVALID 0x1 | PTINVALID 0x1 | FIFOSZ 0x2

Bits | Name | RW | Description
--- | --- | --- | ---
31:12 | RSVD | RO | RESERVED
11 | NRZVALID | RO | 1 Indicates UART/NRZ support.
10 | MANCVALID | RO | 1 Indicates Manchester support.
9 | PTINVALID | RO | 0 Indicates Parallel Trace support.
8:6 | FIFOSZ | RO | FIFO Size reported as a power of two. For instance, 0x3 indicates a FIFO size of 8 bytes.