Name:
=====
 binary_counter


Description:
============
 Example that displays the timer count on the LEDs.


This example increments a variable on every timer interrupt. The global
variable is used to set the state of the LEDs. The example sleeps otherwise.

SWO is configured in 1M baud, 8-n-1 mode.


******************************************************************************


